; # UnicView AD System Configuration File
; # WARNING : Do not modify this file manually! This may render the LCM unusable.
R1=07		; Baudrate: 115200 bps
R5=00		; Custom baudrate divider, high byte
R9=36		; Custom baudrate divider, low byte
R3=5A		; Frame header, high byte
RA=A5		; Frame header, low byte
R6=3F		; ON Brightness
R7=00		; OFF Brightness
R8=05		; SLEEP Time, in seconds
R2=0F
R4=00		; Rotation: Clockwise0
RC=32
RD=00
RE=00

